{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Data_Input"],"not_rendered":{"charts":2,"images":0,"macros":1,"external_links":2,"defined_names":44,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Data_Input","index":0,"n_rows":137,"n_cols":39,"rows_kept":137,"cut":false,"hidden":false,"merged":[[36,37,36,38],[121,26,122,26],[135,15,135,16],[136,15,136,16],[131,15,131,17],[134,15,134,16],[115,27,116,27],[115,26,116,26],[87,19,88,19],[84,15,84,17],[77,15,77,17],[80,15,80,17],[81,15,81,17],[78,15,78,17],[122,16,122,20],[123,16,123,20],[82,15,82,17],[83,15,83,17],[110,5,110,6],[111,5,111,6],[112,5,112,6],[113,5,113,6],[109,1,111,4],[112,1,113,4],[132,15,132,16],[133,15,133,16],[121,25,122,25],[121,24,123,24],[127,10,128,10],[120,10,120,11],[119,10,119,11],[118,10,118,11],[117,10,117,11],[124,16,124,20],[125,16,125,20],[126,16,126,20],[127,16,127,20],[121,15,121,20],[107,1,108,6],[109,5,109,6],[36,30,36,31],[36,32,36,33],[100,10,100,11],[101,10,101,11],[102,10,102,11],[103,10,103,11],[96,12,96,13],[97,12,97,13],[98,12,98,13],[99,12,99,13],[100,12,100,13],[101,12,101,13],[102,12,102,13],[103,12,103,13],[96,10,96,11],[97,10,97,11],[98,10,98,11],[87,20,87,21],[87,22,87,23],[87,24,87,25],[87,26,87,27],[87,15,93,17],[102,6,102,7],[103,6,103,7],[96,6,96,7],[96,8,96,9],[97,6,97,7],[98,6,98,7],[99,6,99,7],[100,6,100,7],[101,6,101,7],[99,8,99,9],[100,8,100,9],[101,8,101,9],[102,8,102,9],[103,8,103,9],[97,8,97,9],[98,8,98,9],[99,10,99,11],[88,12,88,13],[84,10,84,11],[87,8,87,9],[86,8,86,9],[85,8,85,9],[92,12,92,13],[90,10,90,11],[91,10,91,11],[92,10,92,11],[84,8,84,9],[89,8,89,9],[88,8,88,9],[94,10,94,11],[88,10,88,11],[89,10,89,11],[85,12,85,13],[86,12,86,13],[87,12,87,13],[89,12,89,13],[90,12,90,13],[91,12,91,13],[93,12,93,13],[94,12,94,13],[93,6,93,7],[93,8,93,9],[93,10,93,11],[82,6,82,7],[83,6,83,7],[84,6,84,7],[85,6,85,7],[86,6,86,7],[87,6,87,7],[88,6,88,7],[89,6,89,7],[90,6,90,7],[91,6,91,7],[92,6,92,7],[85,10,85,11],[86,10,86,11],[87,10,87,11],[99,1,99,3],[76,15,76,17],[82,1,82,3],[97,1,97,3],[98,1,98,3],[75,11,76,11],[94,6,94,7],[94,8,94,9],[92,8,92,9],[83,8,83,9],[82,8,82,9],[82,10,82,11],[83,10,83,11],[95,15,95,17],[91,8,91,9],[90,8,90,9],[75,4,76,4],[75,1,76,1],[77,9,77,10],[77,7,77,8],[75,7,76,10],[75,2,76,2],[75,3,76,3],[81,6,81,7],[1,23,1,27],[81,8,81,9],[83,12,83,13],[84,12,84,13],[1,1,3,21],[81,10,81,11],[81,12,81,13],[82,12,82,13],[79,15,79,17],[2,23,2,27]]}
[]
[null,"PSC BEAM GIRDER BRIDGE - Korean Roadway Bridge Standard (2016)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MAPI-KEY :"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"base URL :","https://moa-engineers.midasit.com:443/civil"]
[]
[]
[null,"Geometry"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Symbol","Unit","Values",null,null,null,null,"Area","Permeter","Notaional"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L1","m",{"$f":"P47+R63/2+I63+ROUND(AA40/2/TAN(RADIANS(AA31)),3)","v":30.252000000000006},null,null,null,"TypGirder",{"$f":"AA40*AA43+(AA40+AA42)*AA44/2+AA42*AA45+(AA41+AA42)*AA46/2+AA41*AA47","v":0.67140000000000011},{"$f":"AA40+AA43*2+SQRT(AA44^2+((AA40-AA42)/2)^2)*2+AA45*2+SQRT(AA46^2+((AA41-AA42)/2)^2)*2+AA47*2+AA41","v":5.8950696992270322},{"$f":"ROUND(2*AF24/AG24,4)","v":0.2278}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"L2","m",{"$f":"P47+R63","v":30.000000000000004},null,null,null,"EndGirder",{"$f":"AA40*AA43+(AA40+AA41)*AA48/2+AA41*AA49","v":1.3273680000000001},{"$f":"AA40+AA43*2+SQRT(AA48^2+((AA40-AA41)/2)^2)*2+AA49*2+AA41","v":5.3865847899614607},0.49280000000000002]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LT","m",{"$f":"AA24*2+AA25","v":90.504000000000019},null,null,null,"MidSlab",{"$f":"AA27*I67","v":0.75600000000000001},{"$f":"AA27*2+I67*2","v":6.7799999999999994},0.223]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B1","m",3.15,null,null,null,"EndSlab",{"$f":"(AA27/2+AA28+AA29)*I67","v":0.64800000000000002},{"$f":"(AA27/2+AA28+AA29)*2+I67*2","v":5.8800000000000008},0.22040000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B2","m",0.625,null,null,null,"Continuity",{"$f":"R62*AA41","v":1.1682000000000001},{"$f":"R62*2+AA41*2","v":4.8600000000000003},0.48070000000000002]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B3","m",0.5,null,null,null,"Slab",{"$f":"I67*1","v":0.24},{"$f":"I67*2+1*2","v":2.48},0.19350000000000001]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"BT","m",{"$f":"AA27*7+AA28*2+AA29*2","v":24.3},null,null,null,"Cross1",{"$f":"(I61+I62)*(I65+I66)","v":1.7000000000000002},{"$f":"(I61+I62)*2+(I65+I66)*2","v":5.7},0.59650000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"R","degree",60,null,null,null,"Cross2",{"$f":"R61*R62","v":1.2389999999999999},{"$f":"R61*2+R62*2","v":4.9399999999999995},0.50160000000000005]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Plan View"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"MIDDLE",null,"END",null,null,null,null,"CONTINUITY"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PSC_A","PSC_B","PSC_A","PSC_B","SLAB1","SLAB2","MATL","PSC_A","PSC_B"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Symbol","Unit","Values",null,null,null,{"$f":"AA43","v":0.18},{"$f":"AA42/2","v":0.1},{"$f":"AE39","v":0.18},{"$f":"AA41/2-AG44","v":0.32900000000000001},{"$f":"AA27","v":3.15},{"$f":"AA27/2+AA28+AA29","v":2.7},{"$f":"ROUNDUP(G88/K88,4)","v":1.0828},{"$f":"AG39","v":0.18},{"$f":"AH39","v":0.32900000000000001}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SB1","m",0.7,null,null,null,{"$f":"AA44","v":0.1},{"$f":"AA40/2","v":0.35},{"$f":"AA48","v":8.3999999999999995E-3},{"$f":"AA40/2","v":0.35},{"$f":"I67","v":0.24},{"$f":"I67","v":0.24},{"$f":"ROUNDUP(G87/K87,4)","v":1},{"$f":"AG40","v":8.3999999999999995E-3},{"$f":"AH40","v":0.35}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Symbol","Unit","Values",null,null,null,null,null,null,null,null,"SB2","m",0.66,null,null,null,0,0,0,0,null,null,{"$f":"ROUNDUP(G89,4)","v":0.16669999999999999},{"$f":"AG41","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"G1","m",1,null,null,null,null,null,null,null,null,"SB3","m",0.2,null,null,null,0,0,0,0,null,null,{"$f":"ROUNDUP(K89,4)","v":0.16669999999999999},{"$f":"AG42","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"G2","m",3.4,null,null,null,null,null,null,null,null,"SH1","m",0.18,null,null,null,{"$f":"AA45","v":1.27},{"$f":"AA41/2","v":0.33},{"$f":"AA49-AA47-AG44","v":1.5806000000000002},{"$f":"AA41/2","v":0.33},null,null,{"$f":"ROUNDUP(G90/K90,4)","v":1},{"$f":"R62-AL40-AL39-AL47-AL44","v":1.3506000000000002},0.33]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"G3","m",10.17,null,null,null,null,null,null,null,null,"SH2","m",0.1,null,null,null,{"$f":"AA46","v":0.22},0,1E-3,0,null,null,null,{"$f":"AG44","v":1E-3},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"G4","m",0.23,null,null,null,null,null,null,null,null,"SH3","m",1.27,null,null,null,0,0,0,0,null,null,null,{"$f":"AG45","v":0},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"G5","m",0.15,null,null,null,null,null,null,null,null,"SH4","m",0.22,null,null,null,0,null,0,null,null,null,null,{"$f":"AG46","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"GT","m",{"$f":"SUM(P42:P46)*2","v":29.900000000000002},null,null,null,null,null,null,null,null,"SH5","m",0.23,null,null,null,{"$f":"AA47","v":0.23},null,{"$f":"AA47","v":0.23},null,null,null,null,{"$f":"AG47","v":0.23}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"BR","m",0.4,null,null,null,null,null,null,null,null,"SH6","m",8.3999999999999995E-3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"BH","m",0.4,null,null,null,null,null,null,null,null,"SH7","m",{"$f":"AA50-AA48-AA43","v":1.8116000000000001}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ST","m",{"$f":"SUM(AA43:AA47)","v":2}]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Girder"]
[]
[]
[]
[]
[null,null,null,null,null,null,"Symbol","Unit","Values",null,null,null,null,null,null,"Symbol","Unit","Values",null,null,null,null,null,null,"Symbol","Unit","Values"]
[null,null,null,null,null,null,"ET1","m",0.3,null,null,null,null,null,null,"CB","m",0.7,null,null,null,null,null,null,"CR","m",0.53]
[null,null,null,null,null,null,"ET2","m",0.55000000000000004,null,null,null,null,null,null,"CH","m",1.77,null,null,null,null,null,null,"CD","m",0.21629999999999999]
[null,null,null,null,null,null,"[Min] EB","m",0.1,null,null,null,null,null,null,"IG","m",0.1,null,null,null,null,null,null,"TK","m",8.0000000000000002E-3]
[null,null,null,null,null,null,"EB at Center","m",{"$f":"ROUND(AA40/2/TAN(RADIANS(AA31)),3)+I63","v":0.30200000000000005},null,null,null,null,null,null,"TS","m",{"$f":"I67","v":0.24},null,null,null,null,null,null,"TS","m",{"$f":"R64","v":0.24}]
[null,null,null,null,null,null,"EH1","m",0.16]
[null,null,null,null,null,null,"EH2","m",{"$f":"AA50-I65","v":1.84}]
[null,null,null,null,null,null,"TS","m",0.24]
[null,null,null,null,null,null,"BR","m",{"$f":"P48","v":0.4}]
[]
[]
[]
[null,null,null,null,null,"Cross Beam (End)",null,null,null,null,null,null,null,null,"Cross Beam (Pier)",null,null,null,null,null,null,null,null,"Cross Beam (Middle)"]
[]
[null,"Unit",null,null,null,null,"Structure Type",null,null,null,null,null,null,null,null,"Prestressing Layout"]
[]
[null,"Force","Distance","Heat","Temperature",null,"Type","Mass Control Parameter",null,null,null,"Mass\n(Self.W)","Gravity Acc","Initial Temp.",null,"Prestressing Tendon",null,null,"Unit","Values"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(C78=\"mm\",\"[mm/sec²]\",IF(C78=\"cm\",\"[cm/sec²]\",IF(C78=\"m\",\"[m/sec²]\",IF(C78=\"in\",\"[in/sec²]\",IF(C78=\"ft\",\"[ft/sec²]\")))))","v":"[m/sec²]"},{"$f":"IF(E78=\"C\",\"[C]\",IF(E78=\"F\",\"[F]\"))","v":"[C]"},null,"Ultimate Strength",null,null,"MPa",1860]
[null,"kN","m","kcal","C",null,"3-D","Lumped Mass",null,"No option",null,"Convert to X-Y-Z",{"$f":"IF(C78=\"mm\",9806,IF(C78=\"cm\",980.6,IF(C78=\"m\",9.806,IF(C78=\"in\",386.063,IF(C78=\"ft\",32.1719)))))","v":9.8059999999999992},0,null,"Yield Strength",null,null,"MPa",1580]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tendon area",null,null,"mm2",{"$f":"98.71*12","v":1184.52}]
[null,"Materials",null,null,null,null,null,null,null,null,null,null,null,null,null,"Sheath diameter",null,null,"mm",66]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Curvature Friction Factor",null,null,null,0.19]
[null,"Concrete",null,null,null,"Unit","Girder",null,"Cross Beam",null,"Slab",null,"Slab Dummy",null,null,"Wobble Friction Factor",null,null,"1/m",5.0000000000000001E-3]
[null,"Material ID",null,null,null,null,101,null,102,null,103,null,104,null,null,"Anchorage Slip - Begin",null,null,"mm",6]
[null,"Strength Class",null,null,null,null,"C45",null,"C45",null,"C35",null,"C35",null,null,"Anchorage Slip - End",null,null,"mm",6]
[null,"Characteristic compressive strength",null,null,null,"MPa",{"$f":"RIGHT(G84,2)*1","v":45},null,{"$f":"RIGHT(I84,2)*1","v":45},null,{"$f":"RIGHT(K84,2)*1","v":35},null,{"$f":"RIGHT(M84,2)*1","v":35},null,null,"Relaxations Coefficient",null,null,null,"Ordinary"]
[null,"Mean compressive strength",null,null,null,"MPa",{"$f":"IF(G85<=40,G85+4,IF(G85>=60,G85+6,IF(AND(G85>40,G85<60),2/20*(G85-40)+4+G85)))","v":49.5},null,{"$f":"IF(I85<=40,I85+4,IF(I85>=60,I85+6,IF(AND(I85>40,I85<60),2/20*(I85-40)+4+I85)))","v":49.5},null,{"$f":"IF(K85<=40,K85+4,IF(K85>=60,K85+6,IF(AND(K85>40,K85<60),2/20*(K85-40)+4+K85)))","v":39},null,{"$f":"IF(M85<=40,M85+4,IF(M85>=60,M85+6,IF(AND(M85>40,M85<60),2/20*(M85-40)+4+M85)))","v":39}]
[null,"Slef-Weight Density for defining Elastic Modulus",null,null,null,"kg/m³",2300,null,2300,null,2300,null,2300]
[null,"Concrete Elastic Modulus",null,null,null,"MPa",{"$f":"0.077*G87^1.5*(G86^(1/3))","v":31185.368400312807},null,{"$f":"0.077*I87^1.5*(I86^(1/3))","v":31185.368400312807},null,{"$f":"0.077*K87^1.5*(K86^(1/3))","v":28802.97504964891},null,{"$f":"0.077*M87^1.5*(M86^(1/3))","v":28802.97504964891},null,null,"Tendon Profile & Jacking Stress",null,null,null,"Station","Tendon 01",null,"Tendon 02",null,"Tendon 03",null,"Tendon 04"]
[null,"Poisson's Ratio",null,null,null,null,{"$f":"1/6","v":0.16666666666666666},null,{"$f":"1/6","v":0.16666666666666666},null,{"$f":"1/6","v":0.16666666666666666},null,{"$f":"1/6","v":0.16666666666666666},null,null,null,null,null,null,null,"Horizontal","Vertical","Horizontal","Vertical","Horizontal","Vertical","Horizontal","Vertical"]
[null,"Thermal Coefficient",null,null,null,"1/C",{"$f":"0.00001","v":1.0000000000000001E-5},null,{"$f":"0.00001","v":1.0000000000000001E-5},null,{"$f":"0.00001","v":1.0000000000000001E-5},null,{"$f":"0.00001","v":1.0000000000000001E-5},null,null,null,null,null,null,0.15,0,-0.5,0,-0.91399999999999992,0,-1.3,0,-1.706]
[null,"Weight Density for loading",null,null,null,"kN/m³",{"$f":"G92*$M$78","v":24.514999999999997},null,{"$f":"I92*$M$78","v":24.514999999999997},null,{"$f":"K92*$M$78","v":24.514999999999997},null,{"$f":"M92*$M$78","v":0},null,null,null,null,null,null,2.95,0,-0.94500000000000006,0,-1.254,-9.9000000000000008E-3,-1.5070000000000001,9.9000000000000008E-3,-1.774]
[null,"Mass Density for loading",null,null,null,"kN/m³/g",2.5,null,2.5,null,2.5,null,0,null,null,null,null,null,null,5.95,0,-1.319,0,-1.5389999999999999,-4.2900000000000001E-2,-1.681,4.2900000000000001E-2,-1.831]
[null,"Relative Humidity",null,null,null,"%",70,null,70,null,70,null,70,null,null,null,null,null,null,8.9499999999999993,0,-1.5860000000000001,0,-1.742,-9.6700000000000008E-2,-1.806,9.6700000000000008E-2,-1.8719999999999999]
[null,"Type of Cements",null,null,null,null,"1st Class (Moist Cured)",null,"1st Class (Moist Cured)",null,"1st Class (Moist Cured)",null,"1st Class (Moist Cured)",null,null,null,null,null,null,11.95,0,-1.7469999999999999,0,-1.8639999999999999,-0.1353,-1.88,0.1353,-1.897]
[null,"Age of concrete at the beginning of shrinkage",null,null,null,"days",3,null,3,null,3,null,3,null,null,null,null,null,null,14.95,0,-1.8,0,-1.905,-0.15,-1.905,0.15,-1.905]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Prestressing force",null,null,null,17.95,0,-1.7469999999999999,0,-1.8639999999999999,-0.1353,-1.88,0.1353,-1.897]
[null,"Steel",null,null,null,"Unit","Prestressing",null,"Cross Beam",null,null,null,null,null,null,"Tendon 01",1430,"kN",null,20.95,0,-1.5860000000000001,0,-1.742,-9.6700000000000008E-2,-1.806,9.6700000000000008E-2,-1.8719999999999999]
[null,"Material ID",null,null,null,null,201,null,202,null,null,null,null,null,null,"Tendon 02",1388,"kN",null,23.95,0,-1.319,0,-1.5389999999999999,-4.2900000000000001E-2,-1.681,4.2900000000000001E-2,-1.831]
[null,"Strength Class",null,null,null,null,"SWPC7B",null,"SNT355",null,null,null,null,null,null,"Tendon 03",1342,"kN",null,26.95,0,-0.94500000000000006,0,-1.254,-9.9000000000000008E-3,-1.5070000000000001,9.9000000000000008E-3,-1.774]
[null,"Elastic modulus",null,null,null,"MPa",200000,null,210000,null,null,null,null,null,null,"Tendon 04",1291,"kN",null,29.75,0,-0.5,0,-0.91399999999999992,0,-1.3,0,-1.706]
[null,"Poisson's Ratio",null,null,null,null,0.3,null,0.3]
[null,"Thermal Coefficient",null,null,null,"1/C",1.2E-5,null,1.2E-5,null,null,null,null,null,null,"Vehicle loads"]
[null,"Weight Density",null,null,null,"kN/m³",{"$f":"G104*$M$78","v":76.977099999999993},null,{"$f":"I104*$M$78","v":76.977099999999993}]
[null,"Mass Density",null,null,null,"kN/m³/g",7.85,null,7.85]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.45,null,null,{"$f":"(AA30-P105-V105-AB105)/2","v":11.407000000000002},null,null,0.58599999999999997,null,null,{"$f":"S105","v":11.407000000000002},null,null,{"$f":"P105","v":0.45}]
[null,"Superimposed Dead Loads"]
[]
[null,"Loads",null,null,null,null,null,"y1","y2","Area","Width","Thickness","Unit Weight","Pressure"]
[null,null,null,null,null,null,null,"(m)","(m)","(m2)","(m)","(m)","(kN/m3)","(kN/m2)"]
[null,"Guardrail",null,null,null,"Left side",null,{"$f":"LL_W3/2+LL_W2","v":11.700000000000001},{"$f":"H110+LL_W1","v":12.15},0.41994999999999999,0.45,"-",{"$f":"2.5*9.806","v":24.514999999999997},{"$f":"J110*M110/K110*-1","v":-22.877942777777776}]
[null,null,null,null,null,"Right side",null,{"$f":"I110*-1","v":-12.15},{"$f":"H110*-1","v":-11.700000000000001},0.41994999999999999,0.45,"-",{"$f":"2.5*9.806","v":24.514999999999997},{"$f":"J111*M111/K111*-1","v":-22.877942777777776}]
[null,null,null,null,null,"Middle",null,{"$f":"LL_W3/2*-1","v":-0.29299999999999998},{"$f":"LL_W3/2","v":0.29299999999999998},0.41415000000000002,0.58599999999999997,"-",{"$f":"2.5*9.806","v":24.514999999999997},{"$f":"J112*M112/K112*-1","v":-17.325746160409555}]
[null,"Pavement",null,null,null,"Left side",null,{"$f":"(LL_W3/2+Y105)*-1","v":-11.700000000000001},{"$f":"LL_W3/2*-1","v":-0.29299999999999998},"-","-",{"$f":"M125","v":0.05},{"$f":"2.3*9.806","v":22.553799999999995},{"$f":"L113*M113*-1","v":-1.1276899999999999}]
[null,null,null,null,null,"Right side",null,{"$f":"I113*-1","v":0.29299999999999998},{"$f":"H113*-1","v":11.700000000000001},"-","-",{"$f":"L113","v":0.05},{"$f":"2.3*9.806","v":22.553799999999995},{"$f":"L114*M114*-1","v":-1.1276899999999999}]
[]
[null,"Wind Loads",null,null,null,null,null,null,null,null,null,null,null,null,null,"* Traffic loads on left side/ Right side are considered automatically",null,null,null,null,null,null,null,null,null,null,"Lane width\n(m)","Wheel Spacing (m)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"* KL-510TRK/KL-510LNE"]
[null,null,null,null,null,null,null,null,null,null,"Deck Width (B)",null,{"$f":"AA30","v":24.3},"m",null,null,null,null,null,null,null,null,null,null,null,null,3,1.8]
[null,null,null,null,null,null,null,null,null,null,"Deck Height (D)",null,{"$f":"SUM(M123:M126)","v":3.56},"m"]
[null,null,null,null,null,null,null,null,null,null,"B/D ratio",null,{"$f":"M118/M119","v":6.8258426966292136},null,null,"Construction Stage",null,null,null,null,null,null,null,null,"Elastomeric Bearing"]
[null,null,null,null,null,null,null,null,null,null,"Wind Pressure, p",null,{"$f":"IF(AND(M120>=1,M120<8),(4-0.2*M120),IF(M120>=8,2.4))","v":2.6348314606741572},"kPa"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Construction Stage",null,null,null,null,null,"Duaration","Date",null,"Position","Vertical Stiffness","Horizontal Stiffness"]
[null,null,null,null,null,null,null,null,null,null,"Girder","h1",{"$f":"AA50","v":2},"m",null,"CS1","Active Girder",null,null,null,null,28,28]
[null,null,null,null,null,null,null,null,null,null,"Slab","h2",{"$f":"I67","v":0.24},"m",null,"CS2","Prestressing tendon",null,null,null,null,30,{"$f":"W123+V124","v":58},null,null,"kN/m","kN/m"]
[null,null,null,null,null,null,null,null,null,null,"Pavement","h3",0.05,"m",null,"CS3","Loading Wet Slab Concrete",null,null,null,null,30,{"$f":"W124+V125","v":88},null,"Abutment",378200,1797]
[null,null,null,null,null,null,null,null,null,null,"Guardrail","h4",{"$f":"1.32-0.05","v":1.27},"m",null,"CS4","Active Slab and Cross Beam",null,null,null,null,30,118,null,"Pier",756300,3595]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CS5","Loading SIDL",null,null,null,null,0,118]
[null,null,null,null,null,null,null,null,null,null,"No.","P","e","M",null,"CS6","50 years",null,null,null,null,18250,18368]
[null,null,null,null,null,null,null,null,null,null,null,"(kN/m)","(m)","(kN.m/m)"]
[null,null,null,null,null,null,null,null,null,null,1,{"$f":"SUM(M124:M126)*M121","v":4.1103370786516855},{"$f":"SUM(M124:M126)/2-M124","v":0.54},{"$f":"L130*M130","v":2.2195820224719105},null,"Load Combinations",null,null,null,null,null,null,null,null,"Settlement"]
[null,null,null,null,null,null,null,null,null,null,2,{"$f":"M121*M126","v":3.3462359550561795},{"$f":"M126/2+M125","v":0.68500000000000005},{"$f":"L131*M131","v":2.2921716292134833}]
[null,null,null,null,null,null,null,null,null,null,3,{"$f":"M121*M123","v":5.2696629213483144},{"$f":"M123/2+M124","v":1.24},{"$f":"L132*M132","v":6.5343820224719096},null,"Loads",null,null,"ULS","SLS 1","SLS 3","SLS 4","SLS 5",null,"Settlement",10,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Dead Load",null,"DC",1.25,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Superimosed dead load",null,"SIDL",1.5,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Traffic Loads",null,"LL",1.8,1,0.8,0,0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Settlement",null,"SD",1,1,1,1,1]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Wind loads",null,"WS",0,0.3,0,0.7,0]