{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["SimpleBeam"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"SimpleBeam","index":0,"n_rows":16,"n_cols":10,"rows_kept":16,"cut":false,"hidden":false,"merged":[[10,6,12,7],[11,1,14,2],[1,1,2,9],[7,1,9,2],[4,1,5,2],[7,6,8,7],[4,6,5,7]]}
[]
[null,"Create Simple Beam"]
[]
[]
[null,"Units",null,"Distance","m",null,"Material Concrete",null,"Standard","EN04(RC)"]
[null,null,null,"Force","kN",null,null,null,"DB","C35/45"]
[]
[null,{"$f":"\"Geometry \" & \"(\" &E5&\")\"","v":"Geometry (m)"},null,"Length",10,null,{"$f":"\"Additional Loads \" & \"(\" & E6 & \"/\" &E5& \")\"","v":"Additional Loads (kN/m)"},null,"Direction","Value"]
[null,null,null,"Height",1,null,null,null,"GZ",-30]
[null,null,null,"Width",0.8]
[null,null,null,null,null,null,"Load Case",null,"Factor","Name"]
[null,"Modeling ID",null,"material",1,null,null,null,1.2,"DL"]
[null,null,null,"section",1,null,null,null,1.5,"SIDL"]
[null,null,null,"start node",1]
[null,null,null,"start elem",1,null,"base URL :","your baseURL hear"]
[null,null,null,null,null,null,"MAPI-Key :","your MAPI-Key hear"]